Project 1:

Read Analog Input 🡪 Write on CAN1 🡪 Read on CAN2 🡪 Set PWM dutycycle of PWM on LED[i]

Press Pushbutton 🡪 Interrupt 🡪 Increase i